# LM Sensors Input Plugin

Collect [lm-sensors](https://en.wikipedia.org/wiki/Lm_sensors) metrics - requires the lm-sensors
package installed.

This plugin collects sensor metrics with the `sensors` executable from the lm-sensor package.

### Configuration:
```
# Monitor sensors, requires lm-sensors package
[[inputs.sensors]]
  ## Remove numbers from field names.
  ## If true, a field name like 'temp1_input' will be changed to 'temp_input'.
  # remove_numbers = true

  ## Timeout is the maximum amount of time that the sensors command can run.
  # timeout = "5s"
```

### Measurements & Fields:
Fields are created dynamically depending on the sensors. All fields are float.

### Tags:

- All measurements have the following tags:
    - chip
    - feature

### Example Output:

#### Default
```
$ telegraf --config telegraf.conf --input-filter sensors --test
* Plugin: sensors, Collection 1
> sensors,chip=power_meter-acpi-0,feature=power1 power_average=0,power_average_interval=300 1466751326000000000
> sensors,chip=k10temp-pci-00c3,feature=temp1 temp_crit=70,temp_crit_hyst=65,temp_input=29,temp_max=70 1466751326000000000
> sensors,chip=k10temp-pci-00cb,feature=temp1 temp_input=29,temp_max=70 1466751326000000000
> sensors,chip=k10temp-pci-00d3,feature=temp1 temp_input=27.5,temp_max=70 1466751326000000000
> sensors,chip=k10temp-pci-00db,feature=temp1 temp_crit=70,temp_crit_hyst=65,temp_input=29.5,temp_max=70 1466751326000000000
```

#### With remove_numbers=false
```
* Plugin: sensors, Collection 1
> sensors,chip=power_meter-acpi-0,feature=power1 power1_average=0,power1_average_interval=300 1466753424000000000
> sensors,chip=k10temp-pci-00c3,feature=temp1 temp1_crit=70,temp1_crit_hyst=65,temp1_input=29.125,temp1_max=70 1466753424000000000
> sensors,chip=k10temp-pci-00cb,feature=temp1 temp1_input=29,temp1_max=70 1466753424000000000
> sensors,chip=k10temp-pci-00d3,feature=temp1 temp1_input=29.5,temp1_max=70 1466753424000000000
> sensors,chip=k10temp-pci-00db,feature=temp1 temp1_crit=70,temp1_crit_hyst=65,temp1_input=30,temp1_max=70 1466753424000000000
```
