# MQTT Producer Output Plugin

This plugin writes to a [MQTT Broker](http://http://mqtt.org/) acting as a mqtt Producer.

```toml
[[outputs.mqtt]]
  ## URLs of mqtt brokers
  servers = ["localhost:1883"]

  ## topic for producer messages
  topic_prefix = "telegraf"

  ## QoS policy for messages
  ##   0 = at most once
  ##   1 = at least once
  ##   2 = exactly once
  qos = 2

  ## username and password to connect MQTT server.
  # username = "telegraf"
  # password = "metricsmetricsmetricsmetrics"

  ## client ID, if not set a random ID is generated
  # client_id = ""

  ## Timeout for write operations. default: 5s
  # timeout = "5s"

  ## Optional TLS Config
  # tls_ca = "/etc/telegraf/ca.pem"
  # tls_cert = "/etc/telegraf/cert.pem"
  # tls_key = "/etc/telegraf/key.pem"
  ## Use TLS but skip chain & host verification
  # insecure_skip_verify = false

  ## When true, metrics will be sent in one MQTT message per flush.  Otherwise,
  ## metrics are written one metric per MQTT message.
  # batch = false

  ## When true, messages will have RETAIN flag set.
  # retain = false

  ## Defines the maximum length of time that the broker and client may not communicate. 
  ## Defaults to 0 which turns the feature off. For version v2.0.12 mosquitto there is a 
  ## [bug](https://github.com/eclipse/mosquitto/issues/2117) which requires keep_alive to be set.
  ## As a reference eclipse/paho.mqtt.golang v1.3.0 defaults to 30.
  # keep_alive = 0

  ## Data format to output.
  # data_format = "influx"
```

### Required parameters:

* `servers`: List of strings, this is for speaking to a cluster of `mqtt` brokers. On each flush interval, Telegraf will randomly choose one of the urls to write to. Each URL should just include host and port e.g. -> `["{host}:{port}","{host2}:{port2}"]`
* `topic_prefix`: The `mqtt` topic prefix to publish to. MQTT outputs send metrics to this topic format "<topic_prefix>/<hostname>/<pluginname>/" ( ex: prefix/web01.example.com/mem)
* `qos`: The `mqtt` QoS policy for sending messages. See https://www.ibm.com/support/knowledgecenter/en/SSFKSJ_9.0.0/com.ibm.mq.dev.doc/q029090_.htm for details.

### Optional parameters:
* `username`: The username to connect MQTT server.
* `password`: The password to connect MQTT server.
* `client_id`: The unique client id to connect MQTT server. If this parameter is not set then a random ID is generated.
* `timeout`: Timeout for write operations. default: 5s
* `tls_ca`: TLS CA
* `tls_cert`: TLS CERT
* `tls_key`: TLS key
* `insecure_skip_verify`: Use TLS but skip chain & host verification (default: false)
* `batch`: When true, metrics will be sent in one MQTT message per flush. Otherwise, metrics are written one metric per MQTT message.
* `retain`: Set `retain` flag when publishing
* `data_format`: [About Telegraf data formats](https://github.com/influxdata/telegraf/blob/master/docs/DATA_FORMATS_OUTPUT.md)
* `keep_alive`: Defines the maximum length of time that the broker and client may not communicate with each other. Defaults to 0 which deactivates this feature. 
