# gNMI (gRPC Network Management Interface) Input Plugin

This plugin consumes telemetry data based on the [gNMI][1] Subscribe method. TLS
is supported for authentication and encryption.  This input plugin is
vendor-agnostic and is supported on any platform that supports the gNMI spec.

For Cisco devices:

It has been optimized to support gNMI telemetry as produced by Cisco IOS XR
(64-bit) version 6.5.1, Cisco NX-OS 9.3 and Cisco IOS XE 16.12 and later.

[1]: https://github.com/openconfig/reference/blob/master/rpc/gnmi/gnmi-specification.md

Please check the [troubleshooting section](#troubleshooting) in case of
problems, e.g. when getting an *empty metric-name warning*!

## Service Input <!-- @/docs/includes/service_input.md -->

This plugin is a service input. Normal plugins gather metrics determined by the
interval setting. Service plugins start a service to listens and waits for
metrics or events to occur. Service plugins have two key differences from
normal plugins:

1. The global or plugin specific `interval` setting may not apply
2. The CLI options of `--test`, `--test-wait`, and `--once` may not produce
   output for this plugin

## Global configuration options <!-- @/docs/includes/plugin_config.md -->

In addition to the plugin-specific configuration settings, plugins support
additional global and plugin configuration settings. These settings are used to
modify metrics, tags, and field or create aliases and configure ordering, etc.
See the [CONFIGURATION.md][CONFIGURATION.md] for more details.

[CONFIGURATION.md]: ../../../docs/CONFIGURATION.md#plugins

## Configuration

```toml @sample.conf
# gNMI telemetry input plugin
[[inputs.gnmi]]
  ## Address and port of the gNMI GRPC server
  addresses = ["10.49.234.114:57777"]

  ## define credentials
  username = "cisco"
  password = "cisco"

  ## gNMI encoding requested (one of: "proto", "json", "json_ietf", "bytes")
  # encoding = "proto"

  ## redial in case of failures after
  # redial = "10s"

  ## gRPC Maximum Message Size
  # max_msg_size = "4MB"

  ## Enable to get the canonical path as field-name
  # canonical_field_names = false

  ## Remove leading slashes and dots in field-name
  # trim_field_names = false

  ## Guess the path-tag if an update does not contain a prefix-path
  ## Supported values are
  ##   none         -- do not add a 'path' tag
  ##   common path  -- use the common path elements of all fields in an update
  ##   subscription -- use the subscription path
  # path_guessing_strategy = "none"

  ## enable client-side TLS and define CA to authenticate the device
  # enable_tls = false
  # tls_ca = "/etc/telegraf/ca.pem"
  ## Minimal TLS version to accept by the client
  # tls_min_version = "TLS12"
  ## Use TLS but skip chain & host verification
  # insecure_skip_verify = true

  ## define client-side TLS certificate & key to authenticate to the device
  # tls_cert = "/etc/telegraf/cert.pem"
  # tls_key = "/etc/telegraf/key.pem"

  ## gNMI subscription prefix (optional, can usually be left empty)
  ## See: https://github.com/openconfig/reference/blob/master/rpc/gnmi/gnmi-specification.md#222-paths
  # origin = ""
  # prefix = ""
  # target = ""

  ## Vendor specific options
  ## This defines what vendor specific options to load.
  ## * Juniper Header Extension (juniper_header): some sensors are directly managed by
  ##   Linecard, which adds the Juniper GNMI Header Extension. Enabling this
  ##   allows the decoding of the Extension header if present. Currently this knob
  ##   adds component, component_id & sub_component_id as additional tags
  # vendor_specific = []

  ## Define additional aliases to map encoding paths to measurement names
  # [inputs.gnmi.aliases]
  #   ifcounters = "openconfig:/interfaces/interface/state/counters"

  [[inputs.gnmi.subscription]]
    ## Name of the measurement that will be emitted
    name = "ifcounters"

    ## Origin and path of the subscription
    ## See: https://github.com/openconfig/reference/blob/master/rpc/gnmi/gnmi-specification.md#222-paths
    ##
    ## origin usually refers to a (YANG) data model implemented by the device
    ## and path to a specific substructure inside it that should be subscribed
    ## to (similar to an XPath). YANG models can be found e.g. here:
    ## https://github.com/YangModels/yang/tree/master/vendor/cisco/xr
    origin = "openconfig-interfaces"
    path = "/interfaces/interface/state/counters"

    ## Subscription mode ("target_defined", "sample", "on_change") and interval
    subscription_mode = "sample"
    sample_interval = "10s"

    ## Suppress redundant transmissions when measured values are unchanged
    # suppress_redundant = false

    ## If suppression is enabled, send updates at least every X seconds anyway
    # heartbeat_interval = "60s"

  ## Tag subscriptions are applied as tags to other subscriptions.
  # [[inputs.gnmi.tag_subscription]]
  #  ## When applying this value as a tag to other metrics, use this tag name
  #  name = "descr"
  #
  #  ## All other subscription fields are as normal
  #  origin = "openconfig-interfaces"
  #  path = "/interfaces/interface/state"
  #  subscription_mode = "on_change"
  #
  #  ## Match strategy to use for the tag.
  #  ## Tags are only applied for metrics of the same address. The following
  #  ## settings are valid:
  #  ##   unconditional -- always match
  #  ##   name          -- match by the "name" key
  #  ##                    This resembles the previsou 'tag-only' behavior.
  #  ##   elements      -- match by the keys in the path filtered by the path
  #  ##                    parts specified `elements` below
  #  ## By default, 'elements' is used if the 'elements' option is provided,
  #  ## otherwise match by 'name'.
  #  # match = ""
  #
  #  ## For the 'elements' match strategy, at least one path-element name must
  #  ## be supplied containing at least one key to match on. Multiple path
  #  ## elements can be specified in any order. All given keys must be equal
  #  ## for a match.
  #  # elements = ["description", "interface"]
```

## Metrics

Each configured subscription will emit a different measurement.  Each leaf in a
GNMI SubscribeResponse Update message will produce a field reading in the
measurement. GNMI PathElement keys for leaves will attach tags to the field(s).

## Example Output

```text
ifcounters,path=openconfig-interfaces:/interfaces/interface/state/counters,host=linux,name=MgmtEth0/RP0/CPU0/0,source=10.49.234.115,descr/description=Foo in-multicast-pkts=0i,out-multicast-pkts=0i,out-errors=0i,out-discards=0i,in-broadcast-pkts=0i,out-broadcast-pkts=0i,in-discards=0i,in-unknown-protos=0i,in-errors=0i,out-unicast-pkts=0i,in-octets=0i,out-octets=0i,last-clear="2019-05-22T16:53:21Z",in-unicast-pkts=0i 1559145777425000000
ifcounters,path=openconfig-interfaces:/interfaces/interface/state/counters,host=linux,name=GigabitEthernet0/0/0/0,source=10.49.234.115,descr/description=Bar out-multicast-pkts=0i,out-broadcast-pkts=0i,in-errors=0i,out-errors=0i,in-discards=0i,out-octets=0i,in-unknown-protos=0i,in-unicast-pkts=0i,in-octets=0i,in-multicast-pkts=0i,in-broadcast-pkts=0i,last-clear="2019-05-22T16:54:50Z",out-unicast-pkts=0i,out-discards=0i 1559145777425000000
```

## Troubleshooting

### Empty metric-name warning

Some devices (e.g. Juniper) report spurious data with response paths not
corresponding to any subscription. In those cases, Telegraf will not be able
to determine the metric name for the response and you get an
*empty metric-name warning*

For example if you subscribe to `/junos/system/linecard/cpu/memory` but the
corresponding response arrives with path
`/components/component/properties/property/...` To avoid those issues, you can
manually map the response to a metric name using the `aliases` option like

```toml
[[inputs.gnmi]]
  addresses     = ["..."]

  [inputs.gnmi.aliases]
    memory = "/components"

  [[inputs.gnmi.subscription]]
    name = "memory"
    origin = "openconfig"
    path = "/junos/system/linecard/cpu/memory"
    subscription_mode = "sample"
    sample_interval = "60s"
```

If this does *not* solve the issue, please follow the warning instructions and
open an issue with the response, your configuration and the metric you expect.

### Missing `path` tag

Some devices (e.g. Arista) omit the prefix and specify the path in the update
if there is only one value reported. This leads to a missing `path` tag for
the resulting metrics. In those cases you should set `path_guessing_strategy`
to `subscription` to use the subscription path as `path` tag.

Other devices might omit the prefix in updates altogether. Here setting
`path_guessing_strategy` to `common path` can help to infer the `path` tag by
using the part of the path that is common to all values in the update.
