# OPC UA Client Listener Input Plugin

This service plugin receives data from an [OPC UA][opcua] server by subscribing
to nodes and events.

⭐ Telegraf v1.25.0
🏷️ iot
💻 all

[opcua]: https://opcfoundation.org/about/opc-technologies/opc-ua/

## Service Input <!-- @/docs/includes/service_input.md -->

This plugin is a service input. Normal plugins gather metrics determined by the
interval setting. Service plugins start a service to listen and wait for
metrics or events to occur. Service plugins have two key differences from
normal plugins:

1. The global or plugin specific `interval` setting may not apply
2. The CLI options of `--test`, `--test-wait`, and `--once` may not produce
   output for this plugin

## Global configuration options <!-- @/docs/includes/plugin_config.md -->

Plugins support additional global and plugin configuration settings for tasks
such as modifying metrics, tags, and fields, creating aliases, and configuring
plugin ordering. See [CONFIGURATION.md][CONFIGURATION.md] for more details.

[CONFIGURATION.md]: ../../../docs/CONFIGURATION.md#plugins

## Secret store support

This plugin supports secrets from secret stores for the `username` and
`password` option.
See the [secret store documentation][SECRETSTORE] for more details on how
to use them.

[SECRETSTORE]: ../../../docs/CONFIGURATION.md#secret-store-secrets

## Configuration

```toml @sample.conf
# Retrieve data from OPCUA devices
[[inputs.opcua_listener]]
  ## Metric name
  # name = "opcua_listener"
  #
  ## OPC UA Endpoint URL
  # endpoint = "opc.tcp://localhost:4840"
  #
  ## Maximum time allowed to establish a connect to the endpoint.
  # connect_timeout = "10s"
  #
  ## Behavior when we fail to connect to the endpoint on initialization. Valid options are:
  ##     "error": throw an error and exits Telegraf
  ##     "ignore": ignore this plugin if errors are encountered
  #      "retry": retry connecting at each interval
  # connect_fail_behavior = "error"
  #
  ## Maximum time allowed for a request over the established connection.
  # request_timeout = "5s"
  #
  # Maximum time that a session shall remain open without activity.
  # session_timeout = "20m"
  #
  ## Preferred locales for the OPC UA session, ordered by priority.
  ## The server returns LocalizedText values in the first supported locale.
  # locales = []
  #
  ## The interval at which the server should at least update its monitored items.
  ## Please note that the OPC UA server might reject the specified interval if it cannot meet the required update rate.
  ## Therefore, always refer to the hardware/software documentation of your server to ensure the specified interval is supported.
  # subscription_interval = "100ms"
  #
  ## Security policy, one of "None", "Basic128Rsa15", "Basic256",
  ## "Basic256Sha256", or "auto"
  # security_policy = "auto"
  #
  ## Security mode, one of "None", "Sign", "SignAndEncrypt", or "auto"
  # security_mode = "auto"
  #
  ## Path to cert.pem. Required when security mode or policy isn't "None".
  ## If cert path is not supplied, self-signed cert and key will be generated.
  # certificate = "/etc/telegraf/cert.pem"
  #
  ## Path to private key.pem. Required when security mode or policy isn't "None".
  ## If key path is not supplied, self-signed cert and key will be generated.
  # private_key = "/etc/telegraf/key.pem"

  ## Path to additional, explicitly trusted certificate for the remote endpoint
  # remote_certificate = "/etc/telegraf/opcua_server_cert.pem"

  ## Authentication Method, one of "Certificate", "UserName", or "Anonymous".  To
  ## authenticate using a specific ID, select 'Certificate' or 'UserName'
  # auth_method = "Anonymous"
  #
  ## Username. Required for auth_method = "UserName"
  # username = ""
  #
  ## Password. Required for auth_method = "UserName"
  # password = ""
  #
  ## Option to select the metric timestamp to use. Valid options are:
  ##     "gather" -- uses the time of receiving the data in telegraf
  ##     "server" -- uses the timestamp provided by the server
  ##     "source" -- uses the timestamp provided by the source
  # timestamp = "gather"
  #
  ## The default timetsamp format is RFC3339Nano
  # Other timestamp layouts can be configured using the Go language time
  # layout specification from https://golang.org/pkg/time/#Time.Format
  # e.g.: json_timestamp_format = "2006-01-02T15:04:05Z07:00"
  #timestamp_format = ""
  #
  #
  ## Client trace messages
  ## When set to true, and debug mode enabled in the agent settings, the OPCUA
  ## client's messages are included in telegraf logs. These messages are very
  ## noisey, but essential for debugging issues.
  # client_trace = false
  #
  ## Include additional Fields in each metric
  ## Available options are:
  ##   DataType -- OPC-UA Data Type (string)
  # optional_fields = []
  #
  ## Node ID configuration
  ## name              - field name to use in the output
  ## id                - OPC UA node ID string (e.g., "ns=0;i=2262" or "nsu=http://...;s=Name")
  ## namespace         - OPC UA namespace of the node (integer value 0 thru 3)
  ## namespace_uri     - OPC UA namespace URI (alternative to namespace for stable references)
  ## identifier_type   - OPC UA ID type (s=string, i=numeric, g=guid, b=opaque)
  ## identifier        - OPC UA ID (tag as shown in opcua browser)
  ## default_tags      - extra tags to be added to the output metric (optional)
  ## monitoring_params - additional settings for the monitored node (optional)
  ##
  ## Use EITHER 'id' OR the combination of 'namespace/namespace_uri' + 'identifier_type' + 'identifier'
  ##
  ## Monitoring parameters
  ## sampling_interval  - interval at which the server should check for data
  ##                      changes (default: 0s)
  ## queue_size         - size of the notification queue (default: 10)
  ## discard_oldest     - how notifications should be handled in case of full
  ##                      notification queues, possible values:
  ##                      true: oldest value added to queue gets replaced with new
  ##                            (default)
  ##                      false: last value added to queue gets replaced with new
  ## data_change_filter - defines the condition under which a notification should
  ##                      be reported
  ##
  ## Data change filter
  ## trigger        - specify the conditions under which a data change notification
  ##                  should be reported, possible values:
  ##                  "Status": only report notifications if the status changes
  ##                            (default if parameter is omitted)
  ##                  "StatusValue": report notifications if either status or value
  ##                                 changes
  ##                  "StatusValueTimestamp": report notifications if either status,
  ##                                          value or timestamp changes
  ## deadband_type  - type of the deadband filter to be applied, possible values:
  ##                  "None": no deadband filter is applied
  ##                  "Absolute": absolute change in a data value to report a notification
  ##                  "Percent": works only with nodes that have an EURange property set
  ##                             and is defined as: send notification if
  ##                             (last value - current value) >
  ##                             (deadband_value/100.0) * ((high–low) of EURange)
  ## deadband_value - value to deadband_type, must be a float value, no filter is set
  ##                  for negative values
  ##
  ## Use either the inline notation or the bracketed notation, not both.
  #
  ## Inline notation using id string (recommended for simplicity)
  # nodes = [
  #   {name="ProductUri", id="ns=0;i=2262"},
  #   {name="ServerState", id="ns=0;i=2259"}
  # ]
  #
  ## Inline notation using individual fields (default_tags and monitoring_params not supported yet)
  # nodes = [
  #   {name="node1", namespace="", identifier_type="", identifier=""},
  #   {name="node2", namespace="", identifier_type="", identifier=""}
  # ]
  #
  ## Bracketed notation using id string
  # [[inputs.opcua_listener.nodes]]
  #   name = "ProductUri"
  #   id = "ns=0;i=2262"
  #   default_tags = { tag1 = "value1", tag2 = "value2" }

  ## Bracketed notation using individual fields
  # [[inputs.opcua_listener.nodes]]
  #   name = "node1"
  #   namespace = ""
  #   identifier_type = ""
  #   identifier = ""
  #   default_tags = { tag1 = "value1", tag2 = "value2" }
  #
  # [[inputs.opcua_listener.nodes]]
  #   name = "node2"
  #   namespace = ""
  #   identifier_type = ""
  #   identifier = ""
  #
  #   [inputs.opcua_listener.nodes.monitoring_params]
  #     sampling_interval = "0s"
  #     queue_size = 10
  #     discard_oldest = true
  #
  #     [inputs.opcua_listener.nodes.monitoring_params.data_change_filter]
  #       trigger = "Status"
  #       deadband_type = "Absolute"
  #       deadband_value = 0.0
  #
  # [[inputs.opcua_listener.nodes]]
  #   name = "node3"
  #   namespace_uri = "http://opcfoundation.org/UA/"
  #   identifier_type = ""
  #   identifier = ""
  #
  ## Node Group
  ## Sets defaults so they aren't required in every node.
  ## Default values can be set for:
  ## * Metric name
  ## * OPC UA namespace
  ## * Identifier
  ## * Default tags
  ## * Sampling interval
  ##
  ## Multiple node groups are allowed
  #[[inputs.opcua_listener.group]]
  ## Group Metric name. Overrides the top level name.  If unset, the
  ## top level name is used.
  # name =
  #
  ## Group default namespace. If a node in the group doesn't set its
  ## namespace, this is used.
  # namespace =
  #
  ## Group default namespace URI. Alternative to namespace for stable references.
  ## If a node in the group doesn't set its namespace_uri, this is used.
  # namespace_uri =
  #
  ## Group default identifier type. If a node in the group doesn't set its
  ## identifier_type, this is used.
  # identifier_type =
  #
  ## Default tags that are applied to every node in this group. Can be
  ## overwritten in a node by setting a different value for the tag name.
  ##   example: default_tags = { tag1 = "value1" }
  # default_tags = {}
  #
  ## Group default sampling interval. If a node in the group doesn't set its
  ## sampling interval, this is used.
  # sampling_interval = "0s"
  #
  ## Node ID Configuration.  Array of nodes with the same settings as above.
  ## Use either the inline notation or the bracketed notation, not both.
  #
  ## Inline notation (default_tags and monitoring_params not supported yet)
  # nodes = [
  #  {name="node1", namespace="", identifier_type="", identifier=""},
  #  {name="node2", namespace="", identifier_type="", identifier=""}
  #]
  #
  ## Bracketed notation
  # [[inputs.opcua_listener.group.nodes]]
  #   name = "node1"
  #   namespace = ""
  #   identifier_type = ""
  #   identifier = ""
  #   default_tags = { tag1 = "override1", tag2 = "value2" }
  #
  # [[inputs.opcua_listener.group.nodes]]
  #   name = "node2"
  #   namespace = ""
  #   identifier_type = ""
  #   identifier = ""
  #
  #   [inputs.opcua_listener.group.nodes.monitoring_params]
  #     sampling_interval = "0s"
  #     queue_size = 10
  #     discard_oldest = true
  #
  #     [inputs.opcua_listener.group.nodes.monitoring_params.data_change_filter]
  #       trigger = "Status"
  #       deadband_type = "Absolute"
  #       deadband_value = 0.0
  #

  ## Multiple event groups are allowed.
  ## Event nodes support both 'id' string format and individual fields.
  # [[inputs.opcua_listener.events]]
  #   ## Polling interval for data collection
  #   # sampling_interval = "10s"
  #   ## Size of the notification queue
  #   # queue_size = 10
  #   ## Node parameter defaults for node definitions below (used when id is not specified)
  #   # namespace = ""
  #   # identifier_type = ""
  #   ## Specifies OPCUA Event sources to filter on
  #   # source_names = ["SourceName1", "SourceName2"]
  #   ## Fields to capture from event notifications.
  #   ## Fields support namespace-qualified names using "ns:name" format
  #   ## (e.g. "2:TEXT01") and nested browse paths using "/" as separator
  #   ## (e.g. "AckedState/Id" or "2:AckedState/0:Id").
  #   fields = ["Severity", "Message", "Time"]
  #
  #   ## Type or level of events to capture from the monitored nodes.
  #   ## Use 'id' string OR individual fields (namespace/identifier_type/identifier)
  #   [inputs.opcua_listener.events.event_type_node]
  #     id = "ns=0;i=2041"
  #     # Or use individual fields:
  #     # namespace = ""
  #     # identifier_type = ""
  #     # identifier = ""
  #
  #   ## Nodes to monitor for event notifications associated with the defined
  #   ## event type. Use 'id' string OR individual fields.
  #   [[inputs.opcua_listener.events.node_ids]]
  #     id = "ns=2;s=EventSource1"
  #     # Or use individual fields:
  #     # namespace = ""
  #     # identifier_type = ""
  #     # identifier = ""

  ## Browse-based discovery
  ## Walks the server's address space using the Browse service and matches
  ## browse paths against glob patterns to discover Variable nodes
  ## automatically. Backwards compatible: when no paths are configured the
  ## existing nodes/group configuration is used unchanged.
  # [inputs.opcua_listener.browse]
  #   ## Starting node for the browse walk. Defaults to the standard Objects
  #   ## folder when empty.
  #   # root = "ns=0;i=85"
  #
  #   ## Maximum tree depth descended below the root. 0 means unlimited.
  #   # depth = 0
  #
  #   ## Maximum number of discovered nodes. 0 means unlimited.
  #   # max_nodes = 0
  #
  #   ## Number of nodes browsed per Browse request. 0 falls back to the
  #   ## built-in default. Lower values reduce per-RPC payload at the cost
  #   ## of more round trips; raise for fast servers and large trees.
  #   # batch_size = 0
  #
  #   ## Pattern-based discovery rules. Each path defines one glob pattern
  #   ## over browse-path segments. Pattern syntax:
  #   ##   *       any single segment (or any chars within a segment)
  #   ##   **      zero or more segments (recursive descent)
  #   ##   ?       single character within a segment
  #   ##   [abc]   character class within a segment
  #   ##   {a,b}   alternation: any of the comma-separated alternatives
  #   ##   \       escapes the next character
  #   ## Multiple paths may be configured; a node matching multiple patterns
  #   ## appears in each matching group.
  #   # [[inputs.opcua_listener.browse.paths]]
  #   #   pattern = "Server/**"
  #   #   name = "server_vars"
  #   #   default_tags = { source = "browse" }

  ## Enable workarounds required by some devices to work correctly
  # [inputs.opcua_listener.workarounds]
  #  ## Set additional valid status codes, StatusOK (0x0) is always considered valid
  #  # additional_valid_status_codes = ["0xC0"]
  #  ## Use unregistered reads instead of registered reads
  #  # use_unregistered_reads = false
```

### Node Configuration

An OPC UA node ID may resemble: "ns=3;s=Temperature". In this example:

- ns=3 is indicating the `namespace` is 3
- s=Temperature is indicting that the `identifier_type` is a string and
  `identifier` value is 'Temperature'
- This example temperature node has a value of 79.0

#### Using `id` String (Recommended)

You can specify nodes using the standard OPC UA node ID string format directly:

```text
{name="temp", id="ns=3;s=Temperature"},
```

This is simpler and matches the format shown in OPC UA browsers.

#### Using Individual Fields

Alternatively, you can specify each component separately:

```text
{name="temp", namespace="3", identifier_type="s", identifier="Temperature"},
```

> [!NOTE]
> Use either `id` OR the combination of
> `namespace`/`namespace_uri` + `identifier_type` + `identifier`.
> Do not mix both formats for the same node.

This node configuration produces a metric like this:

```text
opcua,id=ns\=3;s\=Temperature temp=79.0,Quality="OK (0x0)" 1597820490000000000
```

With 'DataType' entered in Additional Metrics, this node configuration
produces a metric like this:

```text
opcua,id=ns\=3;s\=Temperature temp=79.0,Quality="OK (0x0)",DataType="Float" 1597820490000000000
```

If the value is an array, each element is unpacked into a field
using indexed keys. For example:

```text
opcua,id=ns\=3;s\=Temperature temp[0]=79.0,temp[1]=38.9,Quality="OK (0x0)",DataType="Float" 1597820490000000000
```

#### Namespace Index vs Namespace URI

OPC UA supports two ways to specify namespaces:

1. **Namespace Index** (`namespace`): An integer (0-3 or higher) that references
   a position in the server's namespace array. This is simpler but can change if
   the server is restarted or reconfigured.

2. **Namespace URI** (`namespace_uri`): A string URI that uniquely identifies
   the namespace. This is more stable across server restarts but requires the
   plugin to fetch the namespace array from the server to resolve the URI to an
   index.

**When to use namespace index:**

- For standard OPC UA namespaces (0 = OPC UA, 1 = Local Server)
- When namespace stability is not a concern
- For simpler configuration

**When to use namespace URI:**

- When you need consistent node references across server restarts
- For production environments where namespace indices might change
- When working with vendor-specific namespaces

**Example using namespace URI:**

```toml
[[inputs.opcua_listener.nodes]]
  name = "ServerStatus"
  namespace_uri = "http://opcfoundation.org/UA/"
  identifier_type = "i"
  identifier = "2256"
```

This produces the same node ID internally as:

```toml
[[inputs.opcua_listener.nodes]]
  name = "ServerStatus"
  namespace = "0"
  identifier_type = "i"
  identifier = "2256"
```

Note: You must specify either `namespace` or `namespace_uri`, not both.

#### Group Configuration

Groups can set default values for the namespace (index or URI), identifier type,
tags settings and sampling interval. The default values apply to all the nodes
in the group. If a default is set, a node may omit the setting altogether. This
simplifies node configuration, especially when many nodes share the same
namespace or identifier type.

The output metric will include tags set in the group and the node.  If
a tag with the same name is set in both places, the tag value from the
node is used.

This example group configuration has three groups with two nodes each:

```toml
  # Group 1
  [[inputs.opcua_listener.group]]
    name = "group1_metric_name"
    namespace = "3"
    identifier_type = "i"
    default_tags = { group1_tag = "val1" }
    [[inputs.opcua.group.nodes]]
      name = "name"
      identifier = "1001"
      default_tags = { node1_tag = "val2" }
    [[inputs.opcua.group.nodes]]
      name = "name"
      identifier = "1002"
      default_tags = {node1_tag = "val3"}

  # Group 2
  [[inputs.opcua_listener.group]]
    name = "group2_metric_name"
    namespace = "3"
    identifier_type = "i"
    default_tags = { group2_tag = "val3" }
    [[inputs.opcua.group.nodes]]
      name = "saw"
      identifier = "1003"
      default_tags = { node2_tag = "val4" }
    [[inputs.opcua.group.nodes]]
      name = "sin"
      identifier = "1004"

  # Group 3
  [[inputs.opcua_listener.group]]
    name = "group3_metric_name"
    namespace = "3"
    identifier_type = "i"
    default_tags = { group3_tag = "val5" }
    nodes = [
      {name="name", identifier="1001"},
      {name="name", identifier="1002"},
    ]
```

### Event Configuration

Defining events allows subscribing to events with the specific node IDs and
filtering criteria based on the event type and source. The plugin subscribes to
the specified `event_type` Node-IDs and collects events that meet the defined
criteria. The `node_ids` parameter specifies the nodes to monitor for events
(monitored items). However, the actual subscription is based on the
`event_type_node` determining the events to capture.

#### Event Group Configuration

You can define multiple groups for the event streaming to subscribe to different
event types. Each group allows to specify defaults for `namespace` and
`identifier_type` being overwritten by settings in `node_ids`. The group
defaults for node information will not affected the `event_type_node` setting
and all paramters must be set in this section.

This example group configuration shows how to use group settings:

```toml
# Group 1
[[inputs.opcua_listener.events]]
   sampling_interval = "10s"
   queue_size = "100"
   source_names = ["SourceName1", "SourceName2"]
   fields = ["Severity", "Message", "Time"]

   [inputs.opcua_listener.events.event_type_node]
     namespace = "1"
     identifier_type = "i"
     identifier = "1234"

   [[inputs.opcua_listener.events.node_ids]]
     namespace = "2"
     identifier_type = "i"
     identifier = "2345"

# Group 2
[[inputs.opcua_listener.events]]
   sampling_interval = "10s"
   queue_size = "100"
   namespace = "3"
   identifier_type = "s"
   source_names = ["SourceName1", "SourceName2"]
   fields = ["Severity", "Message", "Time"]

   [inputs.opcua_listener.events.event_type_node]
     namespace = "1"
     identifier_type = "i"
     identifier = "5678"

    node_ids = [
      {identifier="Sensor1"}, // default values will be used for namespace and identifier_type
      {namespace="2", identifier="TemperatureSensor"}, // default values will be used for identifier_type
      {namespace="5", identifier_type="i", identifier="2002"} // no default values will be used
    ]
```

## Browse-based Discovery

Large deployments often expose thousands of nodes that share a regular
naming scheme. Instead of enumerating each node, the
`[inputs.opcua_listener.browse]` section walks the server's address space
with the Browse service and matches discovered Variable nodes against glob
patterns over their browse paths. Discovered nodes are folded into the
existing pipeline, so the configuration stays backwards compatible with any
explicit `nodes` or `group` entries.

```toml
[inputs.opcua_listener.browse]
  # Starting node for the browse walk (default: Objects folder).
  root = "ns=0;i=85"

  # Optional safety limits.
  depth = 10
  max_nodes = 50000

  # Optional per-RPC tuning.
  batch_size = 50

  [[inputs.opcua_listener.browse.paths]]
    pattern = "Plant1/*/MV*"
    name = "motor_valves"
    default_tags = { plant = "plant1" }

  [[inputs.opcua_listener.browse.paths]]
    pattern = "**/Temperature"
    name = "temperatures"
```

### Pattern Syntax

Patterns are compiled by Telegraf's `filter` package with `/` as the segment
separator:

| Token   | Meaning                                              |
|---------|------------------------------------------------------|
| literal | exact string match for one segment                   |
| `*`     | any single segment, or any characters in a segment   |
| `**`    | zero or more segments (recursive descent)            |
| `?`     | single character within a segment                    |
| `[abc]` | character class within a segment                     |
| `{a,b}` | alternation: any of the comma-separated alternatives |
| `\`     | escapes the next character                           |

A node matched by multiple patterns appears in each matching group;
duplicate `(metric_name, field_name, tags)` combinations are rejected at
mapping time.

The `root` option accepts node-ID strings (`ns=N;...`). Path-string form
and namespace-URI (`nsu=...`) form are not currently supported.

> [!NOTE]
> Browse runs on every connect, so address-space changes (nodes added or
> removed, renumbered namespaces) are picked up on reconnect without
> restarting Telegraf.

## Metrics

The metrics collected by this input plugin will depend on the configured
`nodes`, `events` and the corresponding groups.

## Example Output

```text
group1_metric_name,group1_tag=val1,id=ns\=3;i\=1001,node1_tag=val2 name=0,Quality="OK (0x0)" 1606893246000000000
group1_metric_name,group1_tag=val1,id=ns\=3;i\=1002,node1_tag=val3 name=-1.389117,Quality="OK (0x0)" 1606893246000000000
group2_metric_name,group2_tag=val3,id=ns\=3;i\=1003,node2_tag=val4 Quality="OK (0x0)",saw=-1.6 1606893246000000000
group2_metric_name,group2_tag=val3,id=ns\=3;i\=1004 sin=1.902113,Quality="OK (0x0)" 1606893246000000000
```
