# Redfish Input Plugin

The `redfish` plugin gathers metrics and status information about CPU
temperature, fanspeed, Powersupply, voltage, hostname and Location details
(datacenter, placement, rack and room) of hardware servers for which [DMTF's
Redfish](https://redfish.dmtf.org/) is enabled.

Telegraf minimum version: Telegraf 1.15.0

## Global configuration options <!-- @/docs/includes/plugin_config.md -->

In addition to the plugin-specific configuration settings, plugins support
additional global and plugin configuration settings. These settings are used to
modify metrics, tags, and field or create aliases and configure ordering, etc.
See the [CONFIGURATION.md][CONFIGURATION.md] for more details.

[CONFIGURATION.md]: ../../../docs/CONFIGURATION.md#plugins

## Configuration

```toml @sample.conf
# Read CPU, Fans, Powersupply and Voltage metrics of hardware server through redfish APIs
[[inputs.redfish]]
  ## Redfish API Base URL.
  address = "https://127.0.0.1:5000"

  ## Credentials for the Redfish API.
  username = "root"
  password = "password123456"

  ## System Id to collect data for in Redfish APIs.
  computer_system_id="System.Embedded.1"

  ## Metrics to collect
  ## The metric collects to gather. Choose from "power" and "thermal".
  # include_metrics = ["power", "thermal"]

  ## Tag sets allow you to include redfish OData link parent data
  ## For Example.
  ## Thermal data is an OData link with parent Chassis which has a link of Location.
  ## For more info see the Redfish Resource and Schema Guide at DMTFs website.
  ## Available sets are: "chassis.location" and "chassis"
  # include_tag_sets = ["chassis.location"]

  ## Workarounds
  ## Defines workarounds for certain hardware vendors. Choose from:
  ## * ilo4-thermal - Do not pass 0Data-Version header to Thermal endpoint
  # workarounds = []

  ## Amount of time allowed to complete the HTTP request
  # timeout = "5s"

  ## Optional TLS Config
  # tls_ca = "/etc/telegraf/ca.pem"
  # tls_cert = "/etc/telegraf/cert.pem"
  # tls_key = "/etc/telegraf/key.pem"
  ## Use TLS but skip chain & host verification
  # insecure_skip_verify = false
```

## Metrics

- redfish_thermal_temperatures
  - tags:
    - source
    - member_id
    - address
    - name
    - state
    - health
  - fields:
    - reading_celsius
    - upper_threshold_critical
    - upper_threshold_fatal
    - lower_threshold_critical
    - lower_threshold_fatal

- redfish_thermal_fans
  - tags:
    - source
    - member_id
    - address
    - name
    - state
    - health
  - fields:
    - reading_rpm (or) reading_percent
    - upper_threshold_critical
    - upper_threshold_fatal
    - lower_threshold_critical
    - lower_threshold_fatal

- redfish_power_powersupplies
  - tags:
    - source
    - member_id
    - address
    - name
    - state
    - health
  - fields:
    - last_power_output_watts
    - line_input_voltage
    - power_capacity_watts
    - power_input_watts
    - power_output_watts

- redfish_power_voltages (available only if voltage data is found)
  - tags:
    - source
    - member_id
    - address
    - name
    - state
    - health
  - fields:
    - reading_volts
    - upper_threshold_critical
    - upper_threshold_fatal
    - lower_threshold_critical
    - lower_threshold_fatal

## Tag Sets

- chassis.location
  - tags:
    - datacenter (available only if location data is found)
    - rack (available only if location data is found)
    - room (available only if location data is found)
    - row (available only if location data is found)

- chassis
  - tags:
    - chassis_chassistype
    - chassis_manufacturer
    - chassis_model
    - chassis_partnumber
    - chassis_powerstate
    - chassis_sku
    - chassis_serialnumber
    - chassis_state
    - chassis_health

## Example Output

```text
redfish_thermal_temperatures,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=OK,member_id=0,name=CPU1\ Temp,rack=WEB43,row=North,source=web483,state=Enabled reading_celsius=41,upper_threshold_critical=45,upper_threshold_fatal=48 1691270160000000000
redfish_thermal_temperatures,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,member_id=1,name=CPU2\ Temp,rack=WEB43,row=North,source=web483,state=Disabled upper_threshold_critical=45,upper_threshold_fatal=48 1691270160000000000
redfish_thermal_temperatures,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=OK,member_id=2,name=Chassis\ Intake\ Temp,rack=WEB43,row=North,source=web483,state=Enabled upper_threshold_critical=40,upper_threshold_fatal=50,lower_threshold_critical=5,lower_threshold_fatal=0,reading_celsius=25 1691270160000000000
redfish_thermal_fans,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=OK,member_id=0,name=BaseBoard\ System\ Fan,rack=WEB43,row=North,source=web483,state=Enabled lower_threshold_fatal=0i,reading_rpm=2100i 1691270160000000000
redfish_thermal_fans,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=OK,member_id=1,name=BaseBoard\ System\ Fan\ Backup,rack=WEB43,row=North,source=web483,state=Enabled lower_threshold_fatal=0i,reading_rpm=2050i 1691270160000000000
redfish_power_powersupplies,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=Warning,member_id=0,name=Power\ Supply\ Bay,rack=WEB43,row=North,source=web483,state=Enabled line_input_voltage=120,last_power_output_watts=325,power_capacity_watts=800 1691270160000000000
redfish_power_voltages,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=OK,member_id=0,name=VRM1\ Voltage,rack=WEB43,row=North,source=web483,state=Enabled upper_threshold_fatal=15,lower_threshold_critical=11,lower_threshold_fatal=10,reading_volts=12,upper_threshold_critical=13 1691270160000000000
redfish_power_voltages,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=OK,member_id=1,name=VRM2\ Voltage,rack=WEB43,row=North,source=web483,state=Enabled reading_volts=5,upper_threshold_critical=7,lower_threshold_critical=4.5 1691270160000000000
redfish_thermal_temperatures,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=OK,member_id=0,name=CPU1\ Temp,rack=WEB43,row=North,source=web483,state=Enabled upper_threshold_critical=45,upper_threshold_fatal=48,reading_celsius=41 1691270170000000000
redfish_thermal_temperatures,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,member_id=1,name=CPU2\ Temp,rack=WEB43,row=North,source=web483,state=Disabled upper_threshold_critical=45,upper_threshold_fatal=48 1691270170000000000
redfish_thermal_temperatures,address=127.0.0.1,chassis_chassistype=RackMount,chassis_health=OK,chassis_manufacturer=Contoso,chassis_model=3500RX,chassis_partnumber=224071-J23,chassis_powerstate=On,chassis_serialnumber=437XR1138R2,chassis_sku=8675309,chassis_state=Enabled,health=OK,member_id=2,name=Chassis\ Intake\ Temp,rack=WEB43,row=North,source=web483,state=Enabled lower_threshold_critical=5,lower_threshold_fatal=0,reading_celsius=25,upper_threshold_critical=40,upper_threshold_fatal=50 1691270170000000000
```
